|  |  |  |
| --- | --- | --- |
| **REF. GA DWG.  NO.** | HAHTW100-002-GA |   |
| **SERIAL NO.** | P120096-HAHTW |   |   |
| P120097-HAHTW |   |   |
| **QUANTITY** | 1 PER SHIPSET |   |   |
| 2 (TOTAL) |   |   |
|  |   |   |   |
| **RATING** | LOWER & UPPER DRUM |
| **DRUM CAPACITY** | 56 MM DIA. x 1000 M (SWR, 10 LAYERS) |
| **WINDING LOAD** | 100T x 6 M/MIN  (1ST LAYER, 1ST SPEED) |
|  | 50T x 12 M/MIN  (1ST LAYER, 2ND SPEED) |
|  | 25T x 24 M/MIN  (1ST LAYER, 3RD SPEED) |
|  |  |